Drivers
1. Check https://www.peak-system.com/quick/DrvSetup for the latest PEAK CAN driver.
2. Check https://www.ixxat.com/support/file-and-documents-download/drivers/vci-v4-driver for the latest IXXAT USB-to-CAN driver.
3. Check https://www.zlg.cn/can/down/down/id/22.html for the latest ZLG USB-CAN driver.

Installation of ZLG USB-CAN driver:
1. Open device manager;
2. Select the unavailable USB-CAN device symbol;
3. Install driver from local;
4. Browse to the (installation path)\Drivers\USBCAN-E(2E)-U_driver\32bit\usbcan_e_u.inf or (installation path)\Drivers\USBCAN-E(2E)-U_driver\32bit\usbcan_e_u.inf (Base on you PC);
5. Installation completed.